en	From %d Day Ago

en	From %d Years Ago

en	Upper + Lower bytes

en	Down Host Mail

en	Up Host Mail

en	Down Host Cmd

en	Up Host Cmd

en	Auto

en	0 Digits

en	1 Digit

en	Normal User

en	Host Failure Count

en	The number of Polling Intervals at this Host must be Down before Thold logging an error and reporting Host as Down. Default is 0 (use Cacti setting)

en	Consider Unknown Data as Zero

en	When checking Thresholds, if a Data Source returns Unknown Data ('U'), consider the value as zero for the Threshold check. You can also enable log this issue.

en	If checked, when creating at Threshold Template, its Notification Settings will, by default be owned by the Threshold Template.

en	Checking this box will switch Thold from performing inline Notification to using either the Notification Daemon, or notifications performed out of band by the Notification poller.

en	Check this box if you wish Warning Notification List recipients to receive Alert Emails in addition to the Alert Notification list receivers. This case is applicable when Warning Notifications goes to Administrators and Alert Notifications go to Management.

en	Checking this box will enable Threshold Daemon debug when operating from SystemD or through the command line. This change is dynamic and will take effect as soon as the next Threshold loop commences.

en	If the Thold Daemon is found to be down, send out an Email notification at this frequency.

en	Daemon Threads

en	1 Process

en	%d Processes

en	Log action Consider Unknown Data as Zero

en	When 'Consider Unknown Data as Zero' is enabled, log when it occurs

en	Send Email separately for each address

en	If checked, this will cause all Emails to be sent separately for each address.

en	Supported for Notification Lists and the Notification Queue only. If there are Down Device Notifications in a single processing cycle. Send only one Email to Notification List repipients for all Devices.

en	If a large influx of Down Device Notifications come in, Cacti can pause sending out those Notifications for a certain period of time to see if the issue is transient before sending them out. Select the threshold Down Device Notifications before the Pause is Triggered.

en	If you choose to delay Notifications for a large Down Devices Notification inrush, how long are you willing to wait before allowing the notifications to be processed?

en	Status Change Command

en	You may also Associate the Devices Thresholds as well. However, these Device Thresholds will allow the Threshold Notification List to be overwritten.

en	You may also Disassociate the Devices Thresholds as well. However, these Device Thresholds will allow the Threshold Notification List to be overwritten.

en	To disable all notifications from this Notification List, you can simply disable it here.

en	Email Style/Format File

en	Choose the custom html wrapper and CSS file to use. This file contains both html and CSS to wrap around your report. If it contains more than simply CSS, you need to place a special <REPORT> tag inside of the file. This format tag will be replaced by the report content. These files are located in the 'formats' directory.

en	Read Only

en	Notification has been Suspended. Press the Resume button to resume it

en	Notification has been Resumed. Press the Suspend button to suspend it

en	Pending Notifications have been removed from the database. Previously sent notification not purged will remain until they age out.

en	Event Notifications [ Notifications Suspended by User: %s, %s ago ]

en	Topic

en	Processed

en	Suspend

en	Resume

en	Purge

en	The name of the object as defined by the caller.

en	Object ID

en	The Object ID defined by the caller. Generally its unique 'id'.

en	Event Time

en	Has the Notification Event been processed.

en	Did this notification result in an error. Hover on the error column for details.

en	The time in seconds it took to process the event.

en	Not Specified

en	Done

en	Pending

en	Success

en	Alert Hi for %s (%s)

en	Alert Low for %s (%s)

en	Click 'Continue' to Acknowledge the following Threshold(s). Thresholds that do not allows this, or that are not triggered, will be ignored.

en	Click 'Continue' to Resume Notifications for the following Threshold(s). Thresholds that do not allows this, or that are not triggered will be ignored.

en	Click 'Continue' to Suspend Notifications for the following Threshold(s). Thresholds that do not allows this, or that are not triggered will be ignored.

en	External ID

en	The Threshold Type. For Baseline Types: [TIP] refers to the Time In the Past with MIN, MAX, AVG, and LAST from no more than a day in time from that period. [AOT] refers to the Average over the entire Time period. If there is a colon followed by MIN, MAX, AVG, LAST, the Value came from that Consolidation Function.

en	The High Warning / Alert values. NOTE: Baseline values are a percent, all other values are display values that may be modified by a cdef.

en	The Low Warning / Alert values. NOTE: Baseline values are a percent, all other values are display values that may be modified by a cdef.

en	Enabled at Template Level

en	A Threshold must be enabled both at the Template Level and the Threshold level to be checked.

en	Name (Displayed)

en	Name (Format)

en	The Graph End time will be set at the time of triggering. The Graph Start time will be the End Time minus the Graph Timespan.

en	Skip Scaling on HRULEs

en	If Checked, the Scale on the Graph will not be impacted by either the Alert or Warning HRULEs.

en	Numeric values for High and Low Thresholds can include the following suffixes for numbers greater than 1 to 'K', 'M', 'G', 'T', 'P', 'E', 'Z', 'Y', and for numbers less than 1 'm', 'u', 'p', 'f'.

en	If set and Data Source value goes above this number, warning will be triggered. NOTE: This value must be a RAW number. The value displayed on the Graph may be modified by a cdef.

en	If set and Data Source value goes below this number, warning will be triggered. NOTE: This value must be a RAW number. The value displayed on the Graph may be modified by a cdef.

en	If set and Data Source value goes above this number, alert will be triggered. NOTE: This value must be a RAW number. The value displayed on the Graph may be modified by a cdef.

en	If set and Data Source value goes below this number, alert will be triggered. NOTE: This value must be a RAW number. The value displayed on the Graph may be modified by a cdef.

en	The type of Baseline. [TIP] is the Time in Past, [AOT] is the Average over Time. Percentage Deviation is a percentage value from the historical value. Absolute Value is a deviation either above or below the Baseline over that historical value. For the [TIP] Baseline Types, the MIN, MAX, AVG, and LAST will come from no more than a one day time period at that point in time.

en	Consolidation Function

en	Minimum

en	Maximum

en	The Consolidation function to use for the Baseline Type value calculation.

en	Show Units

en	Display units for very large or small numbers.

en	Force Units Suffix

en	If you wish to display a forced unit suffix on the various Threshold pages and Notifications, enter it here. The size is limited to no more than 10 characters.

en	Decimal Digits to Display

en	The number of decimal digits to display for Threshold and Current Values. The default is auto or 2.

en	Upper data source to calculate the total value.

en	Style/Format File

en	Only logging, maint device

en	Impossible threshold: The Alert Trigger Count must be greater or eval to 1!

en	Impossible threshold: The Alert Trigger Count must be less than or equal to the Trigger Count or eval to 1!

en	Impossible threshold: The Warning Trigger Count must be greater or eval to 1!

en	Threshold Template import columns do not match the database schema

en	Errors encountered while attempting to import Threshold Template data.

en	The Threshold will no longer generate Alerts, Notifications, or execute commands.

en	Ack Detail

en	Date

en	Comment Not Found

en	Ack History

en	No Export Rows Found.

en	Upper data source to use to calculate the total value.

en	The High Warning / Alert values. NOTE: Baseline values are a percent, all other values are RAW values not modified by a cdef.

en	The Low Warning / Alert values. NOTE: Baseline values are a percent, all other values are RAW values not modified by a cdef.

en	The file is too big.

en	Incomplete file transfer.

en	No file uploaded.

en	Temporary folder missing.

en	Failed to write file to disk

en	File upload stopped by extension

en	Invalid file extension.